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SPARKER DCCDI - mounting instructions for Yamaha SR500. 
Wiring
Wiring must be done according the table below. The wires of ignition SPARKER DC-CDI has various colors. (see table). Counterpart connectors are included.
	SPARKER DC-CDI
	motorbike
	note

	blue

	black
	ground

	brown
	white/red
	CKPS high speed

	yellow
	white/green
	CKPS low speed

	
	
	

	red
	brown from ignition key switch
	key switched + 12 V

	
	
	

	blue
	black
	ground

	green
	black/white
	KILL SWITCH

	orange
	orange
	ignition coil


residual wires don't connect
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